The algorithm classifies a Bluetooth beacon as being in either the kitchen or living room based on the RSSI value. Specifically,

was calibrated to be the wall between the kitchen and the living room through trial and error.

The RSSI value and room classification is then sent to a Node Red GUI via MQTT.